1’s and 2’s complement of a 8 bit number

LDA 3000h

CMA

STA 3001h

ADI 01

STA 3002h

HLT

Screenshot:

